* PC (program counter) holds address of the next instruction
* IR holds the current instruction
* 72 is the ASCII equivalent of H
* Assembly language
  + Uses mnemonic codes to represent machine language instructions
* Assembler
  + A program that reads each of the instructions in mnemonic form and translates it into the machine-language equivalent